External receiver interface: